|  |  |
| --- | --- |
| Sample | Absorbance |
| 0.2 µg NO2-/ml standard |  |
| 0.4 µg NO2-/ml standard |  |
| 0.6 µg NO2-/ml standard |  |
| 0.8 µg NO2-/ml standard |  |
| 1.0 µg NO2-/ml standard |  |
| Diesel Car Exhaust (upon startup) |  |
| Diesel Car Exhaust (after running 10 min) |  |
| Gasoline Car Exhaust (upon startup) |  |
| Gasoline Car Exhaust (after running 10 minutes) |  |