|  |  |
| --- | --- |
| Sample | Absorbance |
| 0.2 µg NO2-/ml standard | 0.22 |
| 0.4 µg NO2-/ml standard | 0.43 |
| 0.6 µg NO2-/ml standard | 0.60 |
| 0.8 µg NO2-/ml standard | 0.79 |
| 1.0 µg NO2-/ml standard | 1.05 |
| Diesel Car Exhaust (upon startup) | 1.03 |
| Diesel Car Exhaust (after running 10 minutes) | 1.03 |
| Gasoline Car Exhaust (upon startup) | 0.10 |
| Gasoline Car Exhaust (after running 10 minutes) | 0.04 |