
**

*Figure 1 – Slump cone test: (1)-(3) Filling and rodding three layers; (4) Striking concrete level flush with top of the cone; (5) Lifting cone; (6) Measuring slump.*



*Figure 2 – Air entrainment test.*

**

*Figure 3 – Flow table test.*