Table 1. Chamber specifications for abrasion test. HEPA, high efficiency particulate air.

|  |  |
| --- | --- |
| Dimensions | 1000 mm x 1000 mm x 1000 mm (1 m3), Stainless steel |
| Blower (with HEPA filter) | 200 mm x 200 mm x 200, 909 W |
| Pressure sensor | Magenehelic, 0 ~ 100 mmH20 |
| Filter (chamber inlet) | 320 mm x 320 mm x 400 mm, HEPA filter |
| Charcoal (chamber inlet) | Dia. 90 mm x 260 mm |