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Author Questionnaire

1. Microscopy: Does your protocol require the use of a dissecting or stereomicroscope for performing a complex dissection, microinjection technique, or something similar?  Enter Yes or No.  
If Yes, can you record movies/images using your own microscope camera?
Enter Yes or No.  
If your protocol involves microscopy but you are not able to record movies/images with your microscope camera, JoVE will need to use our scope kit. 
If your microscope does not have a camera port, the scope kit will be attached to one of the eyepieces and you will have to perform the procedure using one eye.
Enter make and model of microscope.
If a dissection or stereo microscope is required for your protocol, please list all shots from the script that will be visualized using the microscope (shots are indicated with the 3-digit numbers, like 2.1.1, 2.1.2, etc.).
Click here to list microscope shots, using the shot numbers from the protocol section of the video script.

2. Software: Does the part of your protocol being filmed include step-by-step descriptions of software usage?  Enter Yes or No.
If Yes, we will need you to record using screen recording software.
We recommend using the screen capture program OBS. JoVE’s tutorial for using OBS Studio is provided at this link: https://review.jove.com/v/5848/screen-capture-instructions-for-authors?status=a7854k
As these files are necessary for finalizing your script, please upload all screen-captured video files to your project page as soon as possible.

3. Filming location: Will the filming need to take place in multiple locations?   Enter Yes or No.
If Yes, how far apart are the locations? Click to enter distance between locations.


4. Testimonials (optional): Would you be open to filming two short testimonial statements live during your JoVE shoot? These will not appear in your JoVE video but may be used in JoVE’s promotional materials. Enter Yes or No.  
If Yes, please provide the full name and position (e.g., Director of [Institute Name], Senior Researcher [University Name], etc.) of the author willing to participate.
Enter full author name, Enter author position


To ensure that your script can be filmed in one day, the protocol sections are cumulatively restricted to 55 shots (shots are the 3-digit numbers like 2.1.1, 2.1.2…etc)


Current Protocol Length
Number of Steps: 25
Number of Shots: 55 (22 SC) 

Introduction
Videographer: Obtain headshots for all authors available at the filming location. 

Answers to these questions will become interview statements that you will deliver on camera.
· Answer up to 2 introduction and up to 3 conclusion questions. No more than 5 interview statements will be included in the video.
· Enter the full name of the author who will deliver the statement.
· Speak naturally and avoid reading the lines.
· Answer in full sentences, the questions will not be displayed in the video. 
· Limit the length of each statement to 20 words or fewer.
· Answers will be edited for length, clarity, and consistency with journal style guidelines.

INTRODUCTION:

What is the scope of your research? What questions are you trying to answer? 
1.1. Enter author name.: Click here to answer question. Please write in a style that you will be comfortable memorizing and speaking aloud. Limit length to 20 or fewer words.

What are the most recent developments in your field of research?
1.2. Enter author name: Click here to answer question. Please write in a style that you will be comfortable memorizing and speaking aloud. Limit length to 20 or fewer words.
What technologies are currently used to advance research in your field?
1.3. Enter author name: Click here to answer question. Please write in a style that you will be comfortable memorizing and speaking aloud. Limit length to 20 or fewer words.
What are the current experimental challenges?
1.4. Enter author name: Click here to answer question. Please write in a style that you will be comfortable memorizing and speaking aloud. Limit length to 20 or fewer words.

CONCLUSION:

What significant findings have you established in your field?
1.5. Enter author name: Click here if you choose this question. Please write in a style that you will be comfortable memorizing and speaking aloud. Limit length to 20 or fewer words.

What research gap are you addressing with your protocol?
1.6. Enter author name: Click here if you choose this question. Please write in a style that you will be comfortable memorizing and speaking aloud. Limit length to 20 or fewer words.

What advantage does your protocol offer compared to other techniques?
1.7. Enter author name: Click here if you choose this question. Please write in a style that you will be comfortable memorizing and speaking aloud. Limit length to 20 or fewer words.
How will your findings advance research in your field?
1.8. Enter author name: Click here if you choose this question. Please write in a style that you will be comfortable memorizing and speaking aloud. Limit length to 20 or fewer words.
What new scientific questions have your results paved the way for?
1.9. Enter author name: Click here if you choose this question. Please write in a style that you will be comfortable memorizing and speaking aloud. Limit length to 20 or fewer words.
What questions will future research focus on?
1.10. Enter author name: Click here if you choose this question. Please write in a style that you will be comfortable memorizing and speaking aloud. Limit length to 20 or fewer words.


Videographer: Obtain headshots for all authors available at the filming location.


Protocol  
[bookmark: _Hlk188263998]Please review this section to make sure that it accurately describes your protocol. Use Track Changes when making edits or revisions.
· The two-digit steps (e.g., 2.1., 2.2.) with purple font are the narration.  JoVE is responsible for the narration of the protocol and results.
· Red italics are pronunciation guides indicating how the word will be spoken. 
· Filming should take no more than 10 minutes per step. If a step takes more than 10 minutes, prepare the product for that step in advance.
· The three-digit shots (e.g., 2.1.1., 2.2.2.) are the actions that the videographer will capture. 

2. Sensor Calibration and Setup
Demonstrator: Click here to enter name of demonstrator(s) 

 
2.1. To begin, assemble the sensor module using a non-dispersive infrared carbon dioxide sensor [1] and a combined temperature and humidity probe [2]. Secure both sensors together as a single functional module [3].	Comment by Poornima  G: Authors: As our shot limit is 55 per video, we will skip the optional and troubleshooting parts in the video.
2.1.1. WIDE: Talent laying out all sensor components on a clean workbench.
2.1.2. Talent positioning the non-dispersive infrared carbon dioxide sensor in the assembly.
2.1.3. Talent attaching the combined temperature and humidity probe to complete the sensor module.

2.2. Configure the microcontroller-based data logger by connecting a real-time clock module [1] and installing the secure digital card shield [2]. Ensure that all components are firmly seated on the microcontroller [3].
2.2.1. Talent connecting the real-time clock module to the microcontroller.
2.2.2. Talent mounting the secure digital card shield onto the data logger.
2.2.3. Close-up shot of the fully assembled microcontroller-based data logger.

2.3. Set the logging frequency to one reading every 10 minutes using the data logger configuration interface [1]. Confirm that the selected interval is correctly saved in the system settings [2].
2.3.1. SCREEN: Display the data logger configuration menu and select the logging interval setting.	Comment by Poornima  G: Authors: Is it possible it record this using a screen recording software? If not, our videographer can film the display. Please let me know.
2.3.2. SCREEN: Show the interval set to one reading every 10 minutes and confirm the selection.
[bookmark: _Hlk162020732][bookmark: _Hlk203170338]Authors: Please create screen capture videos of the shots labeled as SCREEN, write a screenshot summary, and upload the files to your project page as soon as possible : https://review.jove.com/account/file-uploader?src=21138683 

2.4. Now, place the assembled sensor module and data logger inside a weather-resistant housing made of polypropylene [1]. Ensure that all wiring is fully insulated and that all connectors are firmly secured [2].
2.4.1. Talent placing the assembled electronics into the polypropylene enclosure.
2.4.2. Close-up shot of insulated wiring inside the housing.

2.5. To test sensor function and perform calibration, place all carbon dioxide and temperature-humidity sensors in a well-ventilated outdoor area [1]. Arrange the sensors so that they are equally exposed to ambient air [2].
2.5.1. Talent positioning multiple sensor modules outdoors in an open, ventilated area.
2.5.2. Shot showing sensors evenly spaced and exposed to open air.

2.6. Now, connect the sensor modules to a stable power source [1], such as a 230-volt alternating current to direct current adapter [2-TXT]. Allow the sensors to stabilize for 10 minutes [3], then record the baseline carbon dioxide concentration of approximately 410 parts per million to verify consistency across devices [4].
2.6.1. Talent connecting the sensor module to the power source.
2.6.2. Close-up shot of the power connection in place. TXT: Alternatively, use a battery bank rated for continuous 24 h operation
2.6.3. Talent placing the powered sensors in a stationary position outdoors.
2.6.4. Display recorded baseline carbon dioxide readings and compare values across devices.

3. Site Selection and Deployment of Sensor Modules

Demonstrator: Click here to enter name of demonstrator(s) 

3.1. Identify contrasting thermal zones within the locality around the building or zone of interest [1].
3.1.1. TEXT ON PLAIN BACKGROUND:
Select two or more urban typologies, such as:
· High-density built-up area
· Adjacent low-density green or shaded area
· Road-facing façade
· Façade with outdoor HVAC heat-rejection units

3.2. Install sensor modules on multiple façades where applicable to capture thermal and pollutant variation [1]. 
3.2.1. Talent mounting sensor modules on different façades of the building.

3.3. Mount the sensor module using stainless steel brackets fixed with masonry screws [1] or using harness ropes anchored to window grills or wall hooks [2]. Confirm that the module is securely attached to the façade [3].
3.3.1. Talent fixing a stainless steel bracket to the wall using masonry screws.
3.3.2. Talent securing the sensor module with harness ropes to a window grill or wall hook.
3.3.3. Close-up shot of the firmly mounted sensor module on the façade.

3.4. Maintain a mounting height between 1 and 2 meters above the local floor level for each façade [1]. Adjust the exact height as needed based on accessibility, available supporting infrastructure, and façade geometry [2].
3.4.1. Talent measuring the mounting height from the local floor level.
3.4.2. Talent adjusting the sensor position to suit façade geometry and access constraints.

3.5. Now, record the directional orientation of each sensor location [1], such as an east-facing façade adjacent to a road [2], and document nearby obstructions including heating, ventilation, and air conditioning units or walls [3].
3.5.1. Talent noting the compass orientation of the mounted sensor.
3.5.2. Shot showing the sensor relative to a road-facing façade.
3.5.3. Talent noting down in a notebook.

3.6. To configure the power supply, connect the sensor module to a continuous power source [1] using a 230-volt alternating current to 12-volt direct current adapter with surge protection [2].
3.6.1. Talent connecting the power adapter to the sensor module.
3.6.2. Close-up shot of the surge-protected power connection.

3.7. Verify sensor output by observing live readings on the display or logger interface [1]. Confirm that the connection is stable and that active data recording is underway [2].
3.7.1. SCREEN: Show live sensor readings displayed on the logger interface.
3.7.2. SCREEN: Display confirmation of stable connection and ongoing data logging.

3.8. Power the data logger to start recording and capture the diurnal measurement cycle [1].
3.8.1. Talent switching on the data logger and confirming power activation.

3.9. Allow the data logger to operate continuously for 24 hours with a data-logging interval of 10-minutes to capture full-day variations in carbon dioxide concentration, temperature, and humidity [1].
3.9.1. SCREEN: Show 24 h data.

3.10. Verify that timestamps remain synchronized across all sensors before deployment [1] and again after deployment [2].
3.10.1. SCREEN: Display the timestamp settings on one sensor logger interface.
3.10.2. SCREEN: Show the timestamps matching in another sensor.

3.11. Now, record the start time and stop time [1] manually in a field logbook to provide redundant backup documentation [2].
3.11.1. Close-up shot of the field logbook as the talent writes the start time.
3.11.2. Shot of the completed logbook entry with date and times recorded.


4. Data Retrieval, Visualization and Quality Control
Demonstrator: Click here to enter name of demonstrator(s) 

4.1. Retrieve the data by safely ejecting the secure digital card from the logger [1]. Insert the card into a card reader [2] and copy the CSV data files into the designated project folder [3].
4.1.1. Talent removing the secure digital card from the data logger.
4.1.2. Talent inserting the secure digital card into a card reader connected to a computer.
4.1.3. SCREEN: Show data files being copied into the project folder on the computer.

4.2. For wireless fidelity-enabled loggers, connect to the local service set identifier [1] and download the log files through the internet protocol-based dashboard [2].
4.2.1. SCREEN: Display the available wireless fidelity networks and select the local service set identifier.
4.2.2. SCREEN: Show the dashboard interface and the log file download process.

4.3. Process the retrieved data using spreadsheet or data analysis software to prepare it for visualization [1].
4.3.1. SCREEN: Show the comma-separated values file opened in data analysis software and basic data processing steps.

4.4. Next, generate a multi-variable line plot showing carbon dioxide concentration and temperature on the primary vertical axis [1], and relative humidity on the secondary vertical axis [2], to allow direct trend comparison [3].
4.4.1. SCREEN: Display the plotting interface with carbon dioxide concentration and temperature assigned to the primary vertical axis.
4.4.2. SCREEN: Show relative humidity assigned to the secondary vertical axis.
4.4.3. SCREEN: Display the completed multi-variable line plot.

4.5. Label the horizontal axis as Time [1], the primary vertical axis as carbon dioxide parts per million and temperature degree Celsius [2], and the secondary vertical axis as relative humidity percent [3].
4.5.1. SCREEN: Show the horizontal axis being labeled as Time.
4.5.2. SCREEN: Show the primary vertical axis label being edited and confirmed.
4.5.3. SCREEN: Show the secondary vertical axis label being edited and confirmed.

4.6. Add a legend to distinguish variables [1] and annotate peak values, typically between 11 and 15 hours, for inter-site comparison [2].
4.6.1. SCREEN: Display the legend identifying carbon dioxide concentration, temperature, and relative humidity.
4.6.2. SCREEN: Show annotations added to peak values on the plot.

4.7. Perform data validation by reviewing the collected dataset for anomalies [1]. Identify and remove outliers or data points flagged due to timestamp irregularities [2] or device communication errors [3].
4.7.1. SCREEN: Display the dataset in data analysis software with all variables BEING highlighted.
4.7.2. SCREEN: Select data points with irregular timestamps.
4.7.3. SCREEN: Remove flagged data points associated with communication errors.

4.8. Finally, recalibrate sensors if post-experiment analysis indicates sensor drift exceeding 3 percent or a variation of more than 10 parts per million [1]. Repeat the baseline calibration procedure in open-air conditions and reacquire data under identical environmental conditions [2].
4.8.1. Talent placing the sensor modules outdoors for baseline calibration.
4.8.2. Shot of sensors operating in open air during recalibration.



Results
Please review this section to make sure that it accurately reflects your findings.
· This section will not be recorded by the videographer. It only includes the figures/tables from your manuscript (called LAB MEDIA). 
· Use Track Changes when making edits or revisions. Ensure the voiceover length is below 200 words. Current word count: 92.
· Please note that the video cannot include voiceover without an accompanying visual.

5. Results 

5.1. External carbon dioxide concentrations were significantly higher at concrete-dominant façades [1] compared to adjacent green façades across all monitored cities [2].
5.1.1. LAB MEDIA: Table 1. Video editor: Highlight the “average CO2“ for “High Concretization” rows in Chennai, Pune, Mumbai and Hyderabad
5.1.2. LAB MEDIA: Table 1. Video editor: Highlight the “average CO2“ for “Green area north” rows in Chennai, Pune, Mumbai and Hyderabad

5.2. In Chennai, elevated carbon dioxide levels at the east façade coincided with higher local temperatures near the sensor compared to the shaded façade [1].
5.2.1. LAB MEDIA: Figure 5. Video editor: Highlight the CO2 (concrete side) line and the temperature (concrete side) line

5.3. In Pune, the difference in carbon dioxide concentration between façades occurred despite only a 1 degree Celsius increase in temperature at the concrete façade [1].
5.3.1. LAB MEDIA: Figure 6. Video editor: Highlight the CO2 (concrete side) line.

5.4. Green zones consistently exhibited lower temperatures, higher humidity, and faster carbon dioxide dispersion rates compared to concretized façades across all sites [1].
5.4.1. LAB MEDIA: Table 1. Video editor: Highlight the “average temperature and average humidity” columns for “Green area north” rows in Chennai, Pune, Mumbai and Hyderabad.


[bookmark: _Hlk215154137][bookmark: _Hlk215844323]NOTE to the Authors:

You have two options for filming and submitting the SCREEN footage:

Option 1: Uploading Separate Clips (Highly Recommended)

Please upload a separate video file for each SCREEN shot (tagged as SCREEN), naming the file according to the shot number (e.g., 2.4.3, 1.5.1, 3.2.1, 3.1.3, etc.).

- Each clip must be a maximum of 20 to 25 seconds to match the voice narration.
- If an action takes longer, provide only the best, most representative 20-25 second segment.



Option 2: Uploading a Single Continuous Video

If you prefer to record all steps together and upload a single video file, that is acceptable. In this case, you must write the precise timestamp for each shot within the script.

For example, if the action described in shot 2.1.2 is present in the file xxx.mp4 and occurs between timestamps 00:30 and 00:45 , then write the following in the script after each shot description or as a comment bubble.
(write the file name and timestamp after each shot): [File name] [Start Time]-[End Time]
 

- Example 	2.1.2  SCREEN: performing ...........action. xxx.mp4 00:30-00:45
1.2.2 SCREEN: cutting the…..........action. xxx.mp4 01:10-01:20

- The duration between the start and end times for each shot must be limited to 20 to 25 seconds.

- If a shot is longer than 25 seconds, choose two short segments (one at the beginning and one at the end) that collectively do not exceed 25 seconds.
- Example: 3.1.1 SCREEN: inserting a needle... xxx.mp4 00:00-00:10 and 02:30-02:40
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