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· 5.1.1 (Open the FX-6000 V1.0 software) 00:00–00:06
· 5.1.2 (Navigate to the regimen assignment interface and configure the Tissue Train Plate (24 mm rectangle LS) with strain testing set to 20% maximum strain) 00:06–00:09
·  5.1.3 (Allow the program to run and monitor the sinusoidal strain waveform) 00:09–00:31
