Sample Screenshot Summary

· 69615_3.7.1.mp4
· 3.7.1 (ImageJ opened with an image loaded) 00:00-00:22

· 69615_3.8.mp4
· 3.8.1 (Draw a line over the scale bar using the Line tool in Fiji ImageJ) 00:00-01:55
· 3.8.2 (Open Analyze > Set Scale, edit the known distance field, and change the unit to micrometers) 01:56-02:27

· 69615_3.9.1.mp4
· 3.9.1 (Navigate to Analyze > Set Measurements in Fiji ImageJ. Check the boxes for Area and Feret’s diameter in the measurements dialog) 00:00-00:29

· 69615_3.9.2.mp4
· 3.9.2 (Use the Polygon Selection tool to trace the boundary of the object. Press the M key to record and display the measurement results) 00:00-01:05

· 69615_4.1.mp4
· 4.1.1 (StoManager1 is launched through the graphical user interface) 00:02-00:24
· 4.1.2 (Input and output directory is selected within StoManager1) 00:25-00:58

· 69615_4.2.mp4
· 4.2.1 (YOLOv8 segmentation checkbox is checked on and off in the model selection panel) 00:05-00:28

· 69615_4.3.mp4
· 4.3.1 (StoManager1 detection process is started and carried out) 00:04-00:34

· 69615_4.4.mp4
· 4.4.1 (Navigation and opening the output directory) 00:54-01:00
· 4.4.2 (Result images are seen on screen, and comma-separated *.csv files are opened and result images are seen) 00:06-00:53 and 01:01-02:08

· 69615_4.5.mp4
· 4.5.1 (Results file is open in MS Excel) 00:06-00:32


