69640 Roy Screenshot Summary
· 69640_Roy_Screenshot1_6.1.1
· 6.1.1 (The gasket-based mechanical sealing strategy was successfully used to obtain a prototype) 0:00 – 0:10
· 69640_Roy_Screenshot2_6.2
· 6.2.1 (The gasket-based configuration sustained pressures up to 239 millimeters of mercury before leakage) 0:00 – 0:07
· 6.2.2 (and showed a low-pressure drop of 3 millimeters of mercury) 0:07 – 0:13 clip

