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Author Questionnaire

1. Microscopy: Does your protocol require the use of a dissecting or stereomicroscope for performing a complex dissection, microinjection technique, or something similar?  No

2. Software: Does the part of your protocol being filmed include step-by-step descriptions of software usage?  Yes
If Yes, we will need you to record using screen recording software.
We recommend using the screen capture program OBS. JoVE’s tutorial for using OBS Studio is provided at this link: https://review.jove.com/v/5848/screen-capture-instructions-for-authors?status=a7854k
As these files are necessary for finalizing your script, please upload all screen-captured video files to your project page as soon as possible.

3. Filming location: Will the filming need to take place in multiple locations?   Yes 
3 Miles

4. Testimonials (optional): Would you be open to filming two short testimonial statements live during your JoVE shoot? These will not appear in your JoVE video but may be used in JoVE’s promotional materials.  No  



Current Protocol Length
Number of Steps: 11
Number of Shots: 28

Introduction
Videographer: Obtain headshots for all authors available at the filming location. 

Authors: Please note that the questions will not appear on screen. Please answer in stand-alone full sentence with sufficient context. The answers have been revised for clarity and word count.

INTRODUCTION:
REQUIRED: Summarize your research focus and the main questions it aims to answer.
1.1. Nicholas Calabrese: This research provides a minimally invasive method for collecting trawl survey data to quantify regional groundfish abundance, distribution, and biomass.
1.1.1. INTERVIEW: Named talent says the statement above in an interview-style shot, looking slightly off-camera.

Describe the research contexts or systems in which this protocol can be applied.
1.2. Kevin Stokesbury: The methods presented here are adaptable, requiring only minor modifications to be applied across various trawl-based data collection contexts.
1.2.1. INTERVIEW: Named talent says the statement above in an interview-style shot, looking slightly off-camera.
CONCLUSION:
What does this protocol allow researchers to study or measure?
1.3. Kevin Stokesbury: This protocol allows researchers to estimate relative or absolute abundance of any species effectively caught in trawls. 
1.3.1. INTERVIEW: Named talent says the statement above in an interview-style shot, looking slightly off-camera.
Describe the most important consideration or challenge when performing this protocol.
1.4. Nicholas Calabrese: A major challenge in this protocol is operating delicate optical equipment in harsh trawl environments, requiring repair expertise and access to spare parts.

1.4.1. INTERVIEW: Named talent says the statement above in an interview-style shot, looking slightly off-camera. 
How can future studies build on this work? Describe the questions or research directions that can be investigated next.
1.5. Kevin Stokesbury: Future studies can improve this protocol by automating video analysis and integrating stereoscopic measurements to enable faster results.
1.5.1. INTERVIEW: Named talent says the statement above in an interview-style shot, looking slightly off-camera.
Videographer: Obtain headshots for all authors available at the filming location.


Protocol  
Videographer: Please always record an audio slate while filming each shot mentioned in the shotlist.

2. Equipment Setup on the Vessel Deck 
Demonstrators: Stephanie Merhoff and Helena Norton 

2.1. To begin, arrange the survey net and pressure-sensitive winch on the vessel’s deck [1]. Attach the survey trawl doors to the vessel’s winch cables [2]. Then, secure the winch to the deck using a temporary weld [3]. 
2.1.1. WIDE: Talent arranging the survey net and winch on the deck.
2.1.2. Talent attaching the trawl doors to the winch cables.
2.1.3. Talent welding the winch to the deck. 

2.2. Next, wire the winch power cable into the vessel’s breaker box to establish a stable electrical supply [1].
2.2.1. Talent wiring the winch power cable into the vessel’s breaker box.

2.3. Attach a cable block to a mount on the vessel’s A-frame or similar support structure [1] and route the coaxial cable through the block toward the stern, positioning it adjacent to the net drum [2- TXT].
2.3.1. Talent attaching a cable block to a mount on the vessel’s A-frame.
2.3.2. Talent routing the coaxial cable through the block towards the stern, positioning it adjacent to the net drum. TXT: Adjust the cable alignment to prevent chafing
2.4. Attach the junction box to the rigid polyethylene cylinder [1]. Then, mount the cameras and lights onto the cylinder [2]. Now, connect the cameras and lights to the junction box using cables fitted with waterproof connectors [3].
2.4.1. Talent attaching the junction box to the polyethylene cylinder.
2.4.2. Talent mounting the cameras and lights onto the polyethylene cylinder.
2.4.3. Talent connecting the cameras and lights to the junction box using cables fitted with waterproof connectors.
3. Wheelhouse Equipment Set-up for Video and Data Capture
3.1. First, secure the computer and monitors to a stable workstation in the wheelhouse [1]. Then, connect the GPS (G-P-S) devices to the computer to enable real-time spatial data acquisition [2]. Connect the net mensuration receiver to the computer [3]. Now, connect cameras and lights to the power in the vessel’s wheelhouse [4].  
3.1.1. [bookmark: _Int_hH0HTOZ4]WIDE: Talent securing the computer and monitors to a stable workstation in the wheelhouse.
3.1.2. Talent connecting GPS devices to the computer ports.
3.1.3. Talent connecting the net mensuration receiver to the computer.
3.1.4. Talent connecting cameras and lights to power in the vessel’s wheelhouse.  

3.2. After verifying proper equipment function, launch the mapping software to display the vessel location [1]. Check if the time and date stamps are correctly displayed in the video recording software [2]. Enter the tow number to be overlayed on video [3]. Now launch the net mensuration sensor software and begin recording the wingspread and doorspread data [4].

3.2.1. SCREEN: The mapping software is being launched and starts displaying the vessel location.  
Authors: Please create screen capture videos of the shots labeled as SCREEN, create a screenshot summary, and upload the files to your project page as soon as possible: https://review.jove.com/account/file-uploader?src=21396103 

3.2.2. SCREEN: Shot of time and date stamps with cursor hovering over them in the recording software.
3.2.3. SCREEN: Tow number is being entered to be overlayed on video.

3.2.4. SCREEN: Show the net mensuration sensor software being launched and recording the wingspread and doorspread data.

3.3. Deploy the net and doors slowly, using the vessel’s hydraulic winches [1]. Now, start recording the video [2]. Turn on the lights after the cylinder enters the water [3].

3.3.1. Talent setting the net and doors out using the vessel’s hydraulic winches. 

3.3.2. SCREEN: Shot of the video recording being switched on.

3.3.3. Talent turning on the lights after the cylinder enters the water. 
Authors: Are the lights controlled via software or manually? If manual, how far is the switch from the computer, and how do the operators coordinate?

4. Video and Data Acquisition for Each Tow and The Subsequent Review

4.1. Once the vessel’s hydraulic winches are locked into position, proceed to record the location and speed data [1-TXT].

4.1.1. SCREEN: Starting data recording for location and speed data once the vessel’s hydraulic winches are locked into position. TXT: Continue to tow for the allotted duration

4.2. Stop recording location and speed data once the vessel’s hydraulic winches are engaged for haul back, indicating the end of the tow [1]. Switch off the lights once the net and doors are hauled back and the lights reach the surface [2-TXT].

4.2.1. SCREEN: Stop recording location and speed data once the vessel’s hydraulic winches are engaged for haul back.

4.2.2. Talent turning off the lights once they reach the surface. TXT: Repeat the entire process to capture video and data at all stations

4.3. After completing the tow, secure the codend of the net using the codend clip [1]. Document the trawl catch aboard the vessel following standardized procedures [2]. 

4.3.1. Shot of crew attaching the codend clip.
4.3.2. TEXT ON A PLAIN BACKGROUND
-     Empty the codend onto the vessel deck
· Sort the catch into baskets by species
· Measure, weigh, and sex a standardized subsample
· Record counts and weights for remaining catch

4.4. Offload all data from the wheelhouse computer to external hard drives [1]. Upload all videos to the annotation software [2]. Trained technicians shall review and annotate all target species and unidentified fish [3].

4.4.1. Shot of the external hard drives connected to the wheelhouse computer during data transfer. Videographer: Please show the data transfer progressing on the computer screen as well.

4.4.2. SCREEN: Display showing the videos being uploaded to the annotation software. 

4.4.3. Technician annotating the target species and unidentified fish. 


Results
5. Results 

5.1. During the 10 days of sampling, 47 usable survey tows were completed [1], including 4 closed codend [2] and 43 open codend tows during daylight hours [3]. 

5.1.1. LAB MEDIA: Table 1 Video editor: Emphasize the two columns Catch (Ind) and Catch (kg) and highlight all rows except those corresponding to 40 and 43. 

5.1.2. LAB MEDIA: Figure 2 Video editor: Emphasize the red dots.
5.1.3. LAB MEDIA: Figure 2 Video editor: Emphasize the blue dots (mostly look like lines). 

5.2. The length-frequency distribution shows that Atlantic cod captured during the survey ranged from 41 to 81 cm [1].
5.2.1. LAB MEDIA: Figure 3 Video Editor: Please show the full graph and then emphasize the right end with length from 41 cm to 81 cm.
 
5.3. The length-weight relationship demonstrates the expected increase in weight with fish length, confirming consistent biological measurements from the cod sampled during the survey [1].
5.3.1. LAB MEDIA: Figure 4 Video Editor: Please show the entire graph and highlight the equation given in the graph (y = 1E-05x2.9778; R² = 0.962).





Ó 2026, Journal of Visualized Experiments		Page 9 of 9
image1.png




