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5.3.2 (Click Set Parameters and then select the Trypan Blue assay type on the automated cell counter) 00:00-00:12 
[bookmark: _GoBack]5.3.3 (Set the minimum diameter: 1 μm, the maximum diameter: 25 μm, the threshold of living cells: 246, the threshold of dead cells: 200) 00:12-00:20
5.3.4 (Apply parameters and select Count.) 00:20-00:31
5.3.5 (The automated cell counter capturing images and identifying live and dead cells.) 00:31-00:41
70464_screenshot_2.mp4 
5.4.1 (The cell viability percentage and viable cell count is displayed on the instrument screen.Click Mark to identify live and dead cells) 00:00-00:12
