● 70582_screenshot_1.mp4 
o 3.8.1 (Open the software and adjust parameters Set the wavelength to 470 nanometers for GCaMP6f and 560 nanometers for jRGECO1a.) 00:04-00:27 

● 70582_screenshot_2.mp4 
o 3.9.1 (Connect the camera, set the sampling rate to 30 fps, name the file, and click photometry) 00:04-00:34 
