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	Shot 3.9.3. – Slight modification due to us changing the software for the machine and the machine itself.
The image shows the powder x-ray diffraction scan range from 5 to 70 degrees AND the 0.5 seconds per step. 
The 0.5 seconds per step part was moved here from shot 3.9.4.
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	Shot 3.9.4. 
Image of the x-ray diffraction acquisition parameters set to a wavelength of 1.54 angstrom
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	Shot 3.10.1.
Image shows the infrared range being set to 615-4000 cm-1
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	Shot 3.10.2. 
Image shows the infrared scan time being set to 1 minute and the number of scans being set to 4.
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	Shot 3.10.3.
Image shows the infrared spectrum being processed by the machine
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