· 70868_screenshot_1.mp4
· 4.5.1 (Show the fluorescence imaging software acquisition settings as the exposure time is being set to 400 ms, the time-lapse interval is being set to 5 s, and the total imaging duration is being set to 10 min.) 00:00 – 00:12
· 4.5.2 (Show the operator clicking the Start Acquisition button and the first fluorescence image appearing in the acquisition window) 00:12 – 00:17

· 70868_screenshot_2.mp4
· 4.5.3 (Show baseline fluorescence images being captured under non-pressurized conditions.) 00:00 – 00:10

· 70868_screenshot_3.mp4
· 4.7.2 (Display dynamic calcium imaging signals.) 00:03 – 00:07

· 70868_screenshot_4.mp4
· 4.8.2 (Shot of exposure time being adjusted to optimize calcium signal acquisition.) 00:04 – 00:13

· 70868_screenshot_5.mp4
· 4.9.1 (Imaging parameters being modified for different probe settings and signal acquisition) 00:02 – 00:14

· 70868_screenshot_6.mp4
· 4.10.1 (Show the GraphPad Prism software interface displaying data from two groups and the corresponding statistical analysis results.) 00:00 – 00:10
