Screenshot Summary:
· 421&422_screenshot_1.mp4
[bookmark: _GoBack]o 4.1.1 (Opening the fiber photomertry system) 00:03-00:14
o 4.1.2 (setting the signal channel to 470 nm, the control channel to 405 nm and the sampling rate to 60 t o100 Hz) 00:15-00:27
· 431&432_screenshot_2.mp4
o 4.2.2 & 4.2.3 was performed continuously in this screenshot.
