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2.10.2 (Open the interrogator software (Enlight): Displays the reflected Bragg wavelength spectrum from the sensor in a broadband interrogator wavelength range of 1510-1590 nm) 00:00-00:20
2.10.3 (The reflected Bragg wavelength being displayed in the Time response window) 00:23-00:35
(The reflected Bragg wavelength is being recorded/saved) 00:35-01:02
(The reflected Bragg wavelength is being displayed in the Time response window) 01:03-01:10
71446_screenshot_2.mp4
	3.1.2 (The Bragg wavelength being recorded during the turning on of the excitation source) 00:04-00:25
71446_screenshot_3.mp4
	3.1.3 (The Bragg wavelength reaching steady state before turning off the excitation source) 00:00-00:15
71446_screenshot_4.mp4
	3.2.2 (The Bragg wavelength being recorded during natural cooling of the excitation source) 00:01-00:29
71446_screenshot_5.mp4
	3.3.1 (The Bragg wavelength returning to baseline before the next measurement condition is selected) 00:00-00:16
