Screenshot summary

● 72062_screenshot_1.mp4 
o 2.5.1 (The acquisition software being launched.)
● 72062_screenshot_2.mp4 
[bookmark: OLE_LINK8]o 2.5.2 (Examination menu being opened. PhNR Protocol being selected.)
● 72062_screenshot_3.mp4 
o 4.3.4 (Electrode impedance is being measured.)
● 72062_screenshot_4.mp4 
o 5.1.1 (Patient ID/Eye icon being clicked. Patient information being entered.)
● 72062_screenshot_5.mp4 
o 5.1.2 (Binocular testing being selected.)
● 72062_screenshot_6.mp4 
o 5.3.1 (Electrode impedance values being rechecked.)
● 72062_screenshot_7.mp4 
o 5.3.2 (Exam being clicked to begin the acquisition.)
● 72062_screenshot_8.mp4 
o 5.4.1 (The waveform and the artifact-rejection indicator being monitored continuously.)
● 72062_screenshot_9.mp4 
o 5.6.1 (Waveform recording continuing until a reliable waveform is obtained.) 00:00-00:16
o 5.6.2 (Results being clicked to stop the acquisition.) 00:17-00:23
● 72062_screenshot_10.mp4 
[bookmark: OLE_LINK7]o 5.8.1 (The averaged waveform being displayed.)
● 72062_screenshot_11.mp4 
o 5.8.2 (The a-wave, the b-wave, and the photopic negative response trough being identified on the averaged waveform.) 00:00-00:12
o 5.9.1 (The photopic negative response amplitude being measured. The peak time being measured.) 00:13-00:19

