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Author Questionnaire
1. Microscopy: Does your protocol require the use of a dissecting or stereomicroscope for performing a complex dissection, microinjection technique, or something similar?  No  

2. Software: Does the part of your protocol being filmed include step-by-step descriptions of software usage?  Yes
If Yes, we will need you to record using screen recording software.
We recommend using the screen capture program OBS. JoVE’s tutorial for using OBS Studio is provided at this link: https://review.jove.com/v/5848/screen-capture-instructions-for-authors?status=a7854k
As these files are necessary for finalizing your script, please upload all screen-captured video files to your project page as soon as possible.
Videographer: Please record the computer screen for the shots labeled as SCREEN. The screen should be in focus and the fonts should be clearly visible.

3. Filming location: Will the filming need to take place in multiple locations?   No

4. Testimonials (optional): Would you be open to filming two short testimonial statements live during your JoVE shoot? These will not appear in your JoVE video but may be used in JoVE’s promotional materials. No

Current Protocol Length
Number of Steps:  20
Number of Shots: 40 (9 SC) 

Interviews
Videographer: Obtain headshots for all authors available at the filming location. 

Authors: Please note that the questions will not appear on screen. Please answer in stand-alone full sentence with sufficient context
I have chosen 5 best answers
INTRODUCTION:

REQUIRED: Summarize your research focus and the main questions it aims to answer.
1.1. Yingxiao Wang: We aim to develop ultrasound-controlled cell therapies to activate engineered CAR T cells only where they are needed.
1.1.1. INTERVIEW: Named talent says the statement above in an interview-style shot, looking slightly off-camera

Describe the research gap or limitation in existing methods and how this protocol addresses them.
1.2. Peixiang He: Solid tumor CAR T therapy lacks precise spatial control; this protocol uses focused ultrasound for localized activation.
1.2.1. INTERVIEW: Named talent says the statement above in an interview-style shot, looking slightly off-camera
CONCLUSION:
What does this protocol allow researchers to study or measure?
1.3. Fan Wei: This protocol allows researchers to study ultrasound-triggered CAR T activation and measure tumor response over time.
1.3.1. INTERVIEW: Named talent says the statement above in an interview-style shot, looking slightly off-camera

Describe the most important consideration or challenge when performing this protocol.
1.4. Fan Wei: The key challenge is aligning the ultrasound focus, tumor, and thermocouple for stable, reproducible heating.
1.4.1. INTERVIEW: Named talent says the statement above in an interview-style shot, looking slightly off-camera


How can future studies build on this work? Describe the questions or research directions that can be investigated next.
1.5. Peixiang He: Future studies can adapt this workflow to deeper tumors, other antigens, and image-guided temperature monitoring.
1.5.1. INTERVIEW: Named talent says the statement above in an interview-style shot, looking slightly off-camera


Videographer: Obtain headshots for all authors available at the filming location.

Ethics Title Card
This research has been approved by the Institutional Animal Care and Use Committee at the University of Southern California




Protocol  
Videographer: Please always record an audio slate while filming each shot mentioned in the shotlist.

2. Preparation of the Focused Ultrasound (FUS) System
Demonstrator: Click here to enter name of demonstrator(s)
Authors: Please provide the name after the shoot
2.1. To begin, obtain enriched and expanded Echo-Back-PSMA CAR (P-S-M-A  car) T cells by lentiviral transduction of activated primary human T cells [1-TXT]. Then, inject the pre-activated engineered T cells into the established subcutaneous xenograft tumors in the immunodeficient NSG mice to promote tumor engagement [2]. Authors: Please check if the narration is correct
2.1.1. WIDE: Talent placing the tube with engineered cells on the work bench. TXT: PSMA: Prostate-Specific Membrane Antigen 
CAR: Chimeric Antigen Receptor
2.1.2. Talent intratumorally injecting the mouse with the engineered cells. TXT: See the text protocol for the T cell engineering and mouse injection 
Authors: I have added this step to give full context for the workflow and the results as per our journal guidelines. Please film these steps. You can perform a dummy injection or also share any injection videos that you may already have for this step. 

2.2. Three to four days after T-cell injection, prepare the focused ultrasound system for sonothermal stimulation [1]. Degas a sufficient volume of deionized water overnight using a laboratory vacuum system, to reduce acoustic cavitation [1].
2.2.1. Talent turning on the main power button and showing the FUS system.
2.2.2. Talent placing the flask of deionized water in the laboratory vacuum system for degassing.

2.3. Fill the coupling cone of the focused ultrasound transducer with the degassed water [1-TXT]. Inspect the chamber visually and remove all the visible air bubbles before stimulation [2].
2.3.1. Talent filling the coupling cone with the degassed water. 
2.3.2. Talent inspecting the chamber and removing the air bubbles from the coupling cone.

2.4. Mount the 1 megahertz transducer securely on a manual precision positioning stage [1]. 	Authors: Please check if this is correct
2.4.1. Talent mounting the focused ultrasound transducer on the manual precision positioning stage.
Authors:  Please provide the transducer specifications, so that the narration is complete.
Response:	Custom-made 1MHz transducer
2.5. Connect the function generator to the radiofrequency power amplifier and the amplifier output to the transducer [1]. Then, attach the thermometer and the needle-type thermocouple to the control computer [2].
2.5.1. Talent connecting the function generator to the amplifier and the amplifier output to the transducer.
2.5.2. Talent connecting the thermometer and the needle-type thermocouple to the control computer.

2.6. Turn on the function generator, the amplifier, the thermometer, and the computer before preparing the animal, and verify that all the electrical connections are secure [1].
2.6.1. Talent switching on the instruments and checking that the connections are secure.

3. Mouse Preparation
Demonstrator: Click here to enter name of demonstrator(s)

NOTE to Authors: Please consider the following key points for shots involving live
animals/survival surgery (as applicable) to avoid raising concerns by JoVE’s veterinary
reviewers.
· If lifting the animal by the tail, hold it close to the tail base, not far from it.
· Shave 150% of the area surrounding a surgical site (preferably using a depilatory
· cream). Ensure that there are no skin injuries and no fur in the surgical field.
· Prep the surgical site with both iodine-based scrubs and alcohol.
· Use sterile gloves only for surgery (not examination or non-sterile gloves).
· Make skin incisions with a surgical blade, not scissors.
· Avoid using silk thread for closing skin incisions in survival surgeries.

3.1. Position the anesthetized tumor-bearing mouse laterally on a heating pad maintained at 37 degrees Celsius, with the subcutaneous flank tumor facing upward [1]. Secure the mouse gently with laboratory tape [2].
3.1.1. Talent positioning the anesthetized mouse laterally on the heating pad with the tumor facing upward.
3.1.2. Talent securing the animal with tape.
Authors: Please provide the isoflurane concentration for induction and maintenance of anesthesia, as our veterinary reviewers will ask for this information in the video.
Response: 1.5%
Authors: Is 1.5% isoflurane used for anesthesia induction and also maintenance?

3.2. Shave the hair surrounding the tumor [1]. If necessary, apply a depilatory cream to remove any residual hair, then wipe the skin thoroughly [2]. Clean the exposed skin with an alcohol wipe [3], and mark the tumor center with a fine-tip skin marker [4].
3.2.1. Talent shaving the hair surrounding the tumor.
3.2.2. Talent applying depilatory cream and then wiping the area down thoroughly. 
3.2.3. Talent cleaning the area with an alcohol wipe.
3.2.4. Close-up of Talent marking the center of the tumor on the skin.

4. Thermocouple Placement
4.1. Using a sterile small-gauge needle, create a skin opening approximately 2 to 3 millimeters from the tumor edge [1].
4.1.1. Close-up of Talent creating the skin opening with a sterile needle beside the tumor edge. Authors: Are the needles used in this step and the next step 4.2 the same? Are both 29-gauge needles? Please let me know if I should add this to both steps 4.1 and 4.2

4.2. Insert the needle-type thermocouple through the opening at a shallow angle, approximately parallel to the skin surface [1]. Advance the active tip toward the marked tumor center and position it at approximately the tumor mid-depth [2].
4.2.1. Close-up of Talent inserting the needle-type thermocouple through the skin opening at a shallow angle.
Authors: Please give some specifications of the needle-thermocouple. Example: Gauge, type, etc.  Response: 29 gauge
4.2.2. Close-up of Talent advancing the thermocouple tip toward the center of the tumor.
Authors: During filming, please point out the marked tumor center and the insertion site before inserting the thermocouple.
4.3. Secure the thermocouple with laboratory tape to prevent displacement during stimulation [1]. Then, apply a generous layer of degassed ultrasound gel over the tumor and around the insertion site [2].
4.3.1. Talent securing the thermocouple with laboratory tape.
4.3.2. Talent applying the degassed ultrasound gel over the tumor.


5. Focused Ultrasound Transducer Positioning
5.1. Using the positioning stage, slowly lower the transducer toward the tumor and center the acoustic coupling cone over the tumor mark [1].
5.1.1. Close-up of lowering the transducer toward the tumor and aligning it over the marked tumor using the positioning stage.

5.2. Gently bring the coupling cone membrane into contact with the ultrasound gel and confirm continuous acoustic coupling. Check the interface for air bubbles [1]. Adjust the transducer height and angle until the cone is stable and centered over the target [2].
5.2.1. Close-up of bringing the cone membrane into contact with the ultrasound gel.
5.2.2. Close-up of talent inspecting and then adjusting the transducer height and angle over the target.

6. Proportional-Integral-Derivative (PID)-Controlled Stimulation and Animal Recovery
Demonstrator: Click here to enter name of demonstrator(s)
6.1. Launch the dedicated PID controller software on the control computer [1]. Select or enter the communication ports assigned to the function generator and the thermometer. Verify that both devices are recognized [2].
6.1.1. SCREEN:  The PID controller software being launched on the control computer.
[bookmark: _Hlk204179977]Videographer: Please record the computer screen for the shots labeled as SCREEN. The screen should be in focus and the fonts should be clearly visible.
6.1.2. SCREEN: The communication ports being entered and both devices being recognized. 
Authors: Please create screen capture videos of the shots labeled as SCREEN, write a screenshot summary, and upload the files to your project page as soon as possible:
Response: Do we need this if there is a default setting from the software?
Authors: If the settings are in-built and are default and if these cannot be recorded, we can delete the steps. Please let me know which steps are non-filmable and if you wish to delete any of the steps
6.2. Enter the experiment name, the target temperature, the total stimulation duration, and the maximum input voltage limit [1-TXT]. Then, enter the ultrasound operating parameters, including the acoustic frequency, the pulse repetition period, and the duty factor [2].
6.2.1. SCREEN: The experiment name, the target temperature, the duration, and the voltage limit being entered. 
6.2.2. SCREEN: The acoustic frequency, the pulse repetition period, and the duty factor being entered.
Authors: Should we display the parameters for the above 2 steps as text overlay? Or would you provide the parameters used during the shoot after the filming is over?
Either is fine. We will be using the default setting from the software. 
Authors: Please provide the details in the screen recording 
6.3. Verify that the baseline temperature reading is stable, and click Start to initiate the closed-loop stimulation [1]. Monitor the real-time temperature, elapsed time, output voltage, and system status throughout the procedure [2].
6.3.1. SCREEN: The Start button being clicked to initiate the closed-loop stimulation.
6.3.2. SCREEN: The real-time temperature, elapsed time, and output voltage being monitored.

6.4. The software shuts down immediately if the measured temperature exceeds the predefined safety limit of 45 degrees Celsius, or if the animal moves and the acoustic coupling is lost [1]. Authors: The narration is changed based on your response. Please check if this is correct. Will the software auto-shutdown if the animal moves, or if the acoustic coupling is lost?
6.4.1. SCREEN: The stimulation software terminates stimulation upon noting an increase in temperature.
Authors: Please give us the predefined temperature safety limit, so that we can state the value on screen. 
 Response: <45 Celsius (the software can auto-shut down)

7. Completion of Stimulation and Animal Recovery
7.1. At the end of the programmed period, confirm that the software has terminated the voltage output. If necessary, stop the program manually [1]. Then, raise the transducer away from the animal using the positioning stage [2].
7.1.1. SCREEN: The voltage output being confirmed as terminated at the end of the run (hover the cursor over the required area).
7.1.2. Talent raising the transducer away from the animal using the positioning stage.

7.2. Remove the thermocouple carefully from the tumor [1]. Wipe away the ultrasound gel using warm water and paper towels [2].
7.2.1. Close-up of Talent removing the thermocouple from the tumor.
7.2.2. Talent wiping away the ultrasound gel with warm water and paper towels.

7.3. Finally, remove the securing tape [1] and place the mouse on a warm, clean recovery surface [2]. Monitor the mouse continuously until normal movement resumes, and return it to its home cage only after full recovery [3]. Repeat the localized focused ultrasound stimulation four days after the first treatment [4]. Continue monitoring tumor progression by in vivo bioluminescence imaging every two to three days throughout the treatment period [5]. Authors: Please check the changed narration for the last 2 sentences
7.3.1. Talent removing the securing tape.
7.3.2. Talent placing the mouse on the warm recovery surface.
7.3.3. Talent monitoring the mouse until normal movement resumes and placing the animal in cage.
7.3.4. Reuse 5.1.1 and 5.2.2
7.3.5. Talent placing the animal in the bioluminescence imaging setup or operating the bioluminescence system. Authors: This is a representative shot to provide full context to the results.






Results
8. Results
8.1. The closed-loop feedback system maintained localized hyperthermia at approximately 43 degrees Celsius with limited temperature fluctuation [1].
8.1.1. LAB MEDIA: Figure 3A. Video editor: Please emphasize the flat plateau of the temperature trace at 43 degrees Celsius without deleting other parts

8.2. In a heat shock promoter-driven firefly luciferase reporter tumor model, focused ultrasound significantly increased the reporter activity [1]. Bioluminescence at the stimulated site increased markedly six hours after the treatment [2].
8.2.1. LAB MEDIA: Figure 3B. Video editor: Please emphasize the FUS-positive bar and the P value above it without deleting other parts
8.2.2. LAB MEDIA: Figure 3C. Video editor: Please emphasize the FUS-positive mouse in the After panel without deleting other parts

8.3. In the PSMA-positive prostate tumor model, ultrasound-activated EchoBack CAR T cells sustained tumor suppression [1], whereas the tumor burden progressively increased in mice receiving unmodified T cells [2].
8.3.1. LAB MEDIA: Figure 4C. Video editor: Please emphasize the flat EchoBack block on the right of the plot, then the rising plain T cell block on the left
8.3.2. LAB MEDIA: Figure 4D. Video editor: Please sequentially emphasize the Day 11 to the Day 22 rows of the Plain T column
[bookmark: _Hlk203166143]

Watch this video and apply the settings while capturing the screen to obtain high-quality videos: https://www.youtube.com/watch?v=Y67dM1kKcTE 



[bookmark: _Hlk215154137][bookmark: _Hlk215844323]NOTE to the Authors:

You have two options for filming and submitting the SCREEN footage:

Option 1: Uploading Separate Clips (Highly Recommended)

Please upload a separate video file for each SCREEN shot (tagged as SCREEN), naming the file according to the shot number (e.g., 2.4.3, 1.5.1, 3.2.1, 3.1.3, etc.).

- Each clip must be a maximum of 20 to 25 seconds to match the voice narration.
- If an action takes longer, provide only the best, most representative 20-25 second segment.
- Please do not provide longer clips as we won’t be able to use them.



Option 2: Uploading a Single Continuous Video

If you prefer to record all steps together and upload a single video file, that is acceptable. In this case, you must write the precise timestamp for each shot within the script.

For example, if the action described in shot 2.13.1 is present in the file xxx.mp4 and occurs between timestamps 00:30 and 00:45 , then write the following in the script after each shot description or as a comment bubble.
(write the file name and timestamp after each shot): [File name] [Start Time]-[End Time]
 

- Example 	2.13.1  SCREEN: performing ...........action. xxx.mp4 00:30-00:45
2.13.2, SCREEN: cutting the…..........action. xxx.mp4 01:10-01:20

- The duration between the start and end times for each shot must be limited to 20 to 25 seconds.

- If a shot is longer than 25 seconds, choose two short segments (one at the beginning and one at the end) that collectively do not exceed 25 seconds.
- Example: 3.1.1 SCREEN: inserting a needle... xxx.mp4 00:00-00:10 and 02:30-02:40
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