Sample Screenshot Summary:
· 73566_screenshot_1.mp4
· 5.5.2 (Discover ECHO software: Appropriate imaging channel being set for the corresponding dye – Brightfield, DAPI [Hoechst], TxRed [propidium iodide]) 00:00 – 00:22
· 5.5.3 (Hoechst, propidium iodide, and corresponding brightfield images being acquired at the same organoid position) 00:23 – 00:45
· 73566_screenshot_2.mp4
· 5.7.1 (The Hoechst and propidium iodide TIFF files being imported into ImageJ) 00:00 – 00:06
· 5.7.2 (Each organoid being outlined from the Hoechst image) 00:07 – 00:23
· 5.7.3 (The same propidium iodide intensity threshold being applied to all samples) 00:24 – 00:41
· 5.7.4 (The propidium-iodide-positive area as a percentage of the selected reference area being calculated) 00:42 – 00:55
