⚫ 67152_screenshot_1.mp4
 2.1.2  (Software interface showing the initialization progress of eight cameras) 00:00 - 00:25
 2.1.3  ( Switching to Camera mode and selecting the System Resources panel on the left. Then, selecting the eight cameras) 
00:26 - 00:34
⚫ 67152_screenshot_2.mp4
 2.2.1  (To be uploaded by Authors: Selecting Properties tab and setting the flash intensity to 0.95 to 1, gain to 1x, and grayscale mode to Auto) 00:00 - 00:10
 2.2.2   (STo be uploaded by Authors: Navigating to the Centroid Fitting tab and setting the threshold to 0.2–0.4, minimum circularity ratio to 0.5, and maximum blob height to 50)  00:10 - 00:20
⚫ 67152_screenshot_3.mp4
 2.3.2 (Re-selecting all eight cameras from the toolbar) 
00:00 - 00:03
 2.3.3 (Tools panel with calibration option highlighted. Then, selecting the 5 marker Wand & T-Frame calibration object from the T-frame list) 00:04 - 00:43
⚫ 67152_screenshot_4.mp4
 2.4.1  ( Under the Calibrate Cameras option, the Start button is clicked) 00:00 - 00:18
⚫ 67152_screenshot_5.mp4
 2.5.1  (Switching to 3D Perspective view) 00:00 - 00:02
 2.5.3  (To be uploaded by Authors: Navigating to the Set Volume Origin option in the right panel and clicking the Start button)
00:03 - 00:12
⚫ 67152_screenshot_6.mp4
 2.6.2 (Software interface showing force plate synchronization settings at 1000 Hertz) 00:00 - 00:13
 2.6.3 (Connection confirmation of the platform to the PC)
00:14 - 00:32
⚫ 67152_screenshot_7.mp4
 3.1.2 ( Toolbar highlighting the New Database option being selected. Data Management section with New Patient Classification, New Patient, and New Session options being configured) 00:00 - 00:14
⚫ 67152_screenshot_8.mp4
 3.3.1 (Left toolbar with the Go Live button being clicked. View interface showing the Split Horizontal option being applied and selecting graphics to view trajectory counts) 00:00 - 00:18
⚫ 67152_screenshot_9.mp4
 3.4.1 ( Start button being clicked and data collection being recorded) 00:00 - 00:19
 3.4.2 (Stop button being clicked) 00:20 - 00:32
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