2.15.2.mp4
2.15.2: SCREEN: FOV showing full sample.
00:00-00:18
2.15.3.mp4
	2.15.3.: SCREEN: Transmitted light turned on and exposure time adjusted.
	00:00-00:13
2.15.4.mp4
2.15.4.: SCREEN: Laser wavelength, power, and exposure settings adjusted for the sample.
00:08-00:30
2.16.1.mp4
	2.16.1.: SCREEN: Multiple sample positions selected on the microscope software.
00:00-00:24
2.16.2.mp4
	2.16.2.: SCREEN: Z-stack range being defined for a sample.
00:00-00:30
2.16.3.mp4
	2.16.3.: SCREEN: Time-lapse settings entered and acquisition started.
	00:00-00:21
2.19.1.mp4
2.19.1.: SCREEN: Microscope software showing transmitted light, fluorescence, and time-lapse settings configured.
00:02-00:25
2.19.2.mp4
	2.19.2.: SCREEN: Z-stack parameters set with a 2 micrometer step size.
	00:01-00:12
Note: OBS is accidentally visible in this screen recording. The right z step settings are visible in 2.19.1.mp4 and 2.19.3.mp4 as well. I would propose not to use 2.19.2.mp4.
2.19.3.mp4
	2.19.3.: SCREEN: Acquisition is being  initiated.
	00:02-00:13
