79158_screenshot_1.mp4
3.5.1.	SCREEN: Show the lateral flow assay image open in ImageJ. 00:00-00:10
3.5.2.	SCREEN: Show the Image > Color > Split Channels selection in ImageJ. 00:11-00:23

79158_screenshot_2.mp4
3.6.1.	SCREEN: Show the green channel image selected for test-line intensity analysis. 00:00-00:10
3.6.2.	SCREEN: Show a rectangular ROI of 100 x 10 pixels covering the test line. 00:12-00:27
3.6.3.	SCREEN: Show the same ROI size applied to all strip images. 00:52-01:10

79158_screenshot_3.mp4
3.7.1.	SCREEN: Show measurement of the mean intensity value of the test-line region of interest. 00:00-00:10
3.7.2.	SCREEN: Show selection of an adjacent blank membrane region with the same region of interest size. 00:11-00:13
3.7.3.	SCREEN: Show measurement of the background intensity. 00:14-00:27
3.7.4.	SCREEN: Show calculation of the normalized test-line intensity as test-line intensity minus background intensity. 00:33-01:16
