Screenshot

4.4. Refraction.MOV
4.4.3. (Track corneal reflections and measure refractive power in real time using the continuous measurement mode) 00:00-00:04
4.4.4. (Observe live refractive metrics and timeline data logs, then click Pause to stop recording) 00:05-00:07

5.2. B-Scan.MOV
5.2.3. (Open the ultrasound imaging application and display the live ultrasound scan interface) 00:00-00:12
5.2.4. (Click Measure on the left menu bar to open the measurement tool options) 00:13-00:13
[bookmark: _GoBack]5.2.5. (Select the Distance tool, then place and adjust the reference calipers on the target tissue area to measure the distance) 00:14-00:26
5.2.6. (Confirm the distance measurement value, then save the annotated image to the local gallery or exam file) 00:27-00:28
